Connect power to the Timer Controller.

The LCD Display has three display modes – Power Up, Timer, and Totalizer. 

To Change Display Modes
			Press and hold PGRM key. 
			Display will toggle every 3 seconds to next mode
			Release PGRM key at desired mode

--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------

1. Power Up Mode - Displays support parameters(serial#, model#, phone#, mfg.date) and also some operating parameters
 that are user programmable (Timing-Min/Sec, Sequential-On/Off, Totalizer setup – (Program display to  
 match your meter output settings).

			-------------------------------------------------------------------------------------------------------------------------------------------------
			Press PGRM key momentarily and repeatedly to scroll through and view these parameters quickly.    
			Otherwise, Program display will scroll automatically.
			Program blinking parameters to desired values with the INCR or DECR keys.

			-------------------------------------------------------------------------------------------------------------------------------------------------
			To exit Power Up Mode press and hold PGRM key for approximately 3 seconds.
			Display will advance to Timer mode.

--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------

2. Timer Mode -  Displays Timers and their status (on/off, time remaining)

			To Program Timers
			Press PGRM key momentarily.   A blinking arrow will appear pointing at T1(TIMER1)
			Press INCR or DECR keys momentarily and repeatedly to adjust value.
			Repeat above steps for timers T2, T3, T4, and Cntr(Counter) if applicable
			For FAST set, press and hold INCR or DECR keys. After five counts, digits will change rapidly.
			-------------------------------------------------------------------------------------------------------------------------------------------------

			To Manually Start/Test Timers
			Program timers for desired length of “on” time.
			Press TEST/START key momentarily.
Timers will count down from their preset values and reset.
			WARNING:  120VAC outputs will also be activated. 
LED`s indicate status of outputs that are on.
				       
			-------------------------------------------------------------------------------------------------------------------------------------------------
			To exit Timer Mode press and hold PGRM key for approximately 3 seconds.
			Display will advance to Totalizer mode.

--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------

3. Totalizer Mode -   Displays total counts received(switch closures) from the water meter.  This provides total or individual historical values 
 based on the user’s preference.  No action required to record total input counts received.

			--------------------------------------------------------------------------------------------------------------------------------------------------
			To Adjust Totalizer:
			Press PGRM key momentarily and repeatedly until desired digit blinks.
			Press INCR or DECR keys to adjust value.

			-------------------------------------------------------------------------------------------------------------------------------------------------
			To Clear Totalizer :
			Press and hold INCR and DECR keys simultaneaously

			--------------------------------------------------------------------------------------------------------------------------------------------------
			To exit Totalizer Mode press and hold PGRM key for approximately 3 seconds.
			Display will advance to Power Up Mode.

			--------------------------------------------------------------------------------------------------------------------------------------------------

Operate Timer Controller
Unit is now ready to operate.  
Replace dust cover.  
When input signal arrives from water meter, the timer controller will be activated.